

Open project5 and press OK



Add node with connectivity UDG:



Connect the edges:

A screenshot of a computer

Description automatically generated

Press “Generate routing table” + starting running the simulation up until you get the message that U set is generated and then path will be generated. Run the simulation up until you get the message “path generated”.

A screenshot of a computer error

Description automatically generated

A screenshot of a computer error

Description automatically generated

From here the routing table is generate and we can send messages between node.

Press right click on node and send messages to

A screenshot of a computer

Description automatically generated

You will see in right

A screenshot of a computer

Description automatically generated

It means you pick the from node correclt now need to press on the node that you want message to

A computer screen shot of a grid

Description automatically generated

From there run the simulation until you get the message that the message received.

A screenshot of a message

Description automatically generated